**索引**

0, 22. See also LOW, OFF另见LOW、OFF  
1, 22. See also HIGH, ON另见HIGH、ON  
32-bit datapath, 461 :32位数据通道  
32-bit microprocessor, 454 :32位微处理器  
4004 microprocessor chip, 458, 459 :4004微处理器芯片  
74xx series logic, 583 –587 :74xx系列逻辑电路  
 parts,器件  
 2:1 mux (74157), 5862:1多路选择器  
 3:8 decoder (74138), 5863:8解码器  
 4:1 mux (74153), 5864:1多路选择器  
 AND (7408), 585与门  
 AND3 (7411), 5853输入与门  
 AND4 (7421), 5854输入与门  
 counter (74161, 74163), 586 :计数器  
 FLOP (7474), 583, 585触发器  
 NAND (7400), 585:与非门  
 NOR (7402), 585:或非门  
 NOT (7404), 583:非门  
 OR (7432), 585:或门  
 register (74377), 586:寄存器  
 tristate buffer (74244), 586:三态缓冲器  
 XOR (7486), 585:异或门  
80386 microprocessor chip, 459, 460 :80386微处理器芯片  
80486 microprocessor chip, 460, 461: 80486微处理器芯片  
#define, 627–628   
#include, 628–629. See also Standard libraries另见标准库

A  
Abstraction, 4–5:抽象  
 digital. See Digital abstraction数字，另见数字抽象  
Accumulator, 353:累加器  
Acquisition time. See Sampling time: 采集时间，另见采样时间  
Active low, 74–75低电平有效  
A/D conversion, 531 –533:模拟数字转换  
 registers in, 532寄存器入  
ADCs. See Analog/digital converters  
add, 297  
Adders, 239 –246L加法器  
 carry-lookahead, 241:先行进位  
 carry propagate, 240:进位传播  
 full, 56, 240全  
 half, 240半  
 HDL for, 184, 200:硬件描述语言  
 prefix, 243:前缀  
 ripple-carry, 240:行波进位  
addi, 304  
addiu, 345  
addu, 345  
Addition, 14 –15, 17 –18, 235, 239 –246, 297. See also Adders加法，另见加法器  
 binary, 14–15:二进制  
 floating point, 258 –259:浮点数  
 MIPS instructions, 344 –345, 622:MIPS指令

signed binary, 15–17:带符号二进制数  
Address. See also Memory地址，另见存储器  
 physical, 497–501:物理  
 translation, 497 –500:转换  
 virtual, 497. See also Virtual memory :虚拟，另见虚拟内存  
Addressing modes:寻址方式  
 MIPS, 333–335   
 base, 333 :基址  
 immediate, 333 :立即数  
 PC-relative, 333 –334:相对PC  
pseudo-direct, 334 –335伪直接  
 register-only, 333:寄存器  
 x86, 349  
Advanced Micro Devices (AMD), 296, 375, 457, 460(公司名称)  
Advanced microarchitecture, 444 –458:先进微结构  
 branch prediction. See Branch prediction:分支预测

deep pipelines. See Deep pipelines :深度流水线

heterogeneous multiprocessors. See Heterogeneous multiprocessors:异构多处理器

homogeneous multiprocessors.See Homogeneous multiprocessors:同构型多处理器

multithreading. See Multithreading :多线程  
out-of-order processor. See Out-of-order processor:异步处理器  
registerrenaming. SeeRegisterrenaming:寄存器重命名  
single instruction multiple data. SeeSingleInstructionMultipleData:单指令多数据流

superscalar processor. SeeSuperscalar processor:超标量处理器  
Altera FPGA, 274–279:Altera现场可编程逻辑门阵列  
ALU. See Arithmetic/logical unit:算术逻辑单元  
ALU decoder, 382–384:ALU译码器  
HDL for, 432  
ALUControl, 378, 384  
ALUOp, 382–384  
ALUResult, 378  
ALUSrc, 384  
ALUSrcA, 397  
ALUSrcB, 397  
AMAT. See Average memory access time平均内存访问时间  
AMD. See Advanced Micro Devices   
Amdahl, Gene, 480   
Amdahl’s Law, 480Amdahl定律  
American Standard Code for Information Interchange (ASCII), 322, 323, 630, 649–650美国信息交换标准码

Analog I/O, 531 –537模拟I/O

A/D conversion, 532 –533模/数转换  
D/A conversion, 533–537数/模转换  
Pulse-width modulation (PWM), 脉冲宽度调制536–537  
Analog-to-digital converters (ADCs), 模拟数字转换器531–533  
Analytical engine, 7, 8分析机  
AND gate, 20 –22, 179与门  
chips (7408, 7411, 7421), 585芯片  
truth table, 20, 22真值表  
using CMOS transistors, 32–33使用CMOS晶体管  
and, 311  
andi, 311–312  
AND-OR (AO) gate, 46与或门  
Anode, 27阳极  
Application-specific integrated circuits(ASICs), 591专用集成电路  
Architectural state, 310, 371 –372体系机构状态  
Architecture, 295–356, 619–622体系结构  
 MIPS   
 addressing modes, 333–335编址方式  
 assembly language, 296–304, 619–622汇编语言  
 instructions, 619–622指令  
 machine language, 305–310机器语言  
 operands, 298–304操作数  
 x86, 347–356  
Arguments, 326, 332 –333, 637 参数  
 pass by reference, 644按引用传递  
 pass by value, 644按值传递  
Arithmetic算术  
 C operators, 633–635 C运算符  
 circuits, 239 –254 电路  
 HDL operators, 185 HDL运算符  
 MIPS instructions, 310 –314 MIPS指令  
 packed, 454封装  
Arithmetic/logical unit (ALU), 248 –250, 378算术逻辑单元  
 implementation of, 249 实现  
 in MIPS processor, 382–385.在MIPS处理器中  
 See also ALUControl, ALUOp

Arrays, 320 –324, 645 –651 数组

accessing, 320 –322, 645访问

as input argument, 646–647作为输入参数

bytes and characters, 322 –324, 649–651字节和字符  
comparison or assignment of, 650比较或赋值  
declaration, 645声明  
indexing, 320 –322, 645–649索引  
initialization, 645–646初始化  
multi-dimension, 648–649 多维度  
ASCII. See American Standard Code for Information Interchange美国信息交换标准码  
ASICs. See Application-specific integrated circuits专用集成电路  
Assembler, 338–339, 666汇编器  
Assembler directives, 338汇编器指令  
Assembler temporary register ($at), 342:汇编器临时寄存器  
Assembly language, MIPS, 295–356, 619–622. See also MIPS instructions汇编语言，另见MIPS指令  
instructions, 296 –304, 619 –622:指令  
logical instructions, 311 –312:逻辑指令  
operands, 298 –304:操作数  
translating high-level code into, 300 :转换高级语言代码为  
translating machine language to, 309 :转换机器语言为  
translating to machine language, 306 –307 :转换为机器语言  
Assembly language, x86. See x86instructions汇编语言，另见x86指令  
Associativity结合性  
in Boolean algebra, 62, 63在布尔代数  
in caches, 481, 486–488在缓存中  
Astable circuits, 119:非稳态电路  
Asymmetric multiprocessors. SeeHeterogeneous multiprocessors:非对称多处理器，另见异构多处理器  
Asynchronous circuits, 120 –123:异步电路  
Asynchronous resettable flip-flopsdefinition, 116:异步复位触发器定义  
HDL, 194–196  
Asynchronous serial link, 522. See also Universal Asynchronous Receiver Transmitter (UART) :异步串联，另见通用异步收发器

AT Attachment (ATA), 562:AT附件  
Average memory access time (AMAT), 479, 492:平均内存访问时间

B  
Babbage, Charles, 7   
Base address, 301–302, 307, 320–322, 324 :基址  
Base addressing, 333:基址寻址  
Baud rate register (BRG), 518:波特率寄存器  
BCD. See Binary coded decimal: 二进制编码的十进制数

Behavioral modeling, 173–174 :行为建模  
Benchmarks, 375:基准测试程序  
beq, 314–315  
Biased exponent, 257:偏移指数  
Big-endian memory, 302–303:大端存储器  
Big-endian order, 178 :大端顺序  
Binary addition, 14 –15. See also Adders,Addition :二进制加法，另见加法器、加法  
Binary coded decimal (BCD), 258:二进制编码的十进制数  
Binary encoding, 125–126, 129–131:二进制编码  
for divide-by-3 counter, 129–131:除以3计数器  
for traffic light FSM, 125–126 :交通灯有限状态机  
Binary numbers:二进数  
signed, 15 –19:有符号  
unsigned, 9 –11:无符号  
Binary to decimal conversion, 10, 10 –11:二-十进制转换  
Binary to hexadecimal conversion, 12:二-十六进制转换  
Bipolar junction transistors, 26:双极性晶体管  
Bipolar motor drive, 555:双极电机驱动  
Bipolar signaling, 524:双极性信号  
Bipolar stepper motor, 554, 554–555:双极步进电机  
AIRPAX LB82773-M1, 554, 555  
direct drive current, 556:直流驱动电流  
Bistable element, 109:双稳态元件  
Bit, 8:比特位  
dirty, 494脏  
least significant, 13, 14:最低有效  
most significant, 13, 14:最高有效  
sign, 16:有符号  
use, 490:使用  
valid, 484:有效  
Bit cells, 264 –269:位元  
DRAM, 266–267:动态随机存储器;  
ROM, 268–269:只读存储器  
SRAM, 267:静态随机存储器  
Bitline, 264:位线  
Bit swizzling, 188:位交叉混合  
Bitwise operators, 177 –179:位运算符  
Block, 481 :块  
Block offset, 488–489 :块偏移  
Block size (b), 481, 488–489:块大小  
Blocking and nonblocking assignments, 199 –200, 205–209:阻塞和非阻塞赋值  
BlueSMiRF silver module, 548, 548BlueSMiRF silver模块  
Bluetooth wireless communication, 547–548蓝牙无线通信  
BlueSMiRF silver module, 548BlueSMiRF silver模块  
classes, 547:类别  
PIC32 to PC link, 548: PIC32与PC链接  
bne, 314–315  
Boole, George, 8   
Boolean algebra, 60 –66:布尔代数  
axioms, 61:公理

equation simplification, 65 –66:等式简化

theorems, 61–64:定理  
Boolean equations, 58 –60:布尔等式  
product-of-sums (POS) form, 60:或与式  
sum-of-products (SOP) form, 58 –60:与或式  
Boolean logic, 8. See also Booleanalgebra, Logic gates:布尔逻辑，另见布尔代数、逻辑门  
Boolean theorems, 61–64:布尔定理  
associativity, 63:结合律  
combining, 62:合并律  
complements, 62 :互补定理  
consensus, 62, 64:一致律  
covering, 62:吸收律  
De Morgan’s, 63 –64:德∙摩根定理  
distributivity, 63:分布律  
idempotency, 62:重叠定理  
identity, 62:同一性定理  
involution, 62:回旋定理  
null element, 62:零元定理  
Branch, 384:分支  
Branch equal (beq)

machine code for, 334 机器代码

processor implementations of, 381–382, 395–396, 401–402:处理器实现  
Branch hazards. See Control hazards 分支相关，另见控制相关

Branch misprediction penalty, 421–422:分支预测错误惩罚  
Branch prediction, 446 –447:分支预测  
Branch target address (BTA), 333–334,381:分支目标地址  
Branch target buffer, 446:分支目标缓冲  
Branching分支

conditional, 314 –315:有条件

unconditional (jump), 315 –316:无条件  
Breadboards, 600 –601:电路试验板  
BTA. See Branch target address:分支目标地址  
Bubble, 20, 63, 419气泡  
pushing, 63–64, 71 –73推  
Buffers, 20 :缓冲  
lack of, 117 :缺少  
tristate, 74–75 :三态门  
Bugs, 175: 程序错误  
in C code, 667 –671 :C代码  
Bus, 56:总线  
tristate, 75:三态  
Bypassing, 416. See also Forwarding :绕过  
Byte, 13 –14, 322 –324. See also Character:字节，另见字符  
least significant, 13 –14 :最低有效   
most significant, 13 –14 :最高有效  
Byte-addressable memory, 301 –303:字节寻址存储器  
big-endian, 302 –303 :大端  
little-endian, 302 –303 :小端  
Byte offset, 483:字节偏移

C  
C programming, 623 –671 :C语言编程  
common mistakes. See Common mistakes :常见错误  
compilation. See Compilation:编译  
conditional statements. See Conditional statements:条件语句  
 control-flow statements. See Controlflow statements:控制流语句  
data types. See Data types:数据类型  
function calls. See Function calls:函数调用  
loops. See Loops:循环  
operators. See Operators:操作符  
running, 626:运行  
simple program, 625 –626:简单程序  
standard libraries. See Standardlibraries:标准库  
variables. See Variables :变量  
Caches, 480 –495 :缓存  
address fields, :地址域  
block offset, 488–489:块偏移  
byte offset, 483 :字节偏移  
set bits, 483:设置位  
tag, 483:标签  
advanced design, 491 –495:先进设计  
evolution of, in MIPS, 495 :演化，MIPS内  
multiple level, 492:多层次  
nonblocking, 566:非阻塞  
organizations, 490 :组织  
direct mapped, 482 –486:直接映射  
fully associative, 487 –488:全关联  
multiway set associative, 486 –487:多路设置关联  
parameters:参数  
block, 481 :块  
block size, 481, 488 –489 :块大小  
capacity (C), 480–481:容量  
degree of associativity (N), 486:关联度  
number of sets (S), 481 :集数目  
performance of :性能  
hit, 478–480:命中  
hit rate, 478–480:命中率  
miss, 478–480, 493:缺失  
capacity, 493 :容量  
compulsory, 493:强制  
conflict, 486, 493:冲突  
penalty, 488:惩罚  
miss rate, 478 –480:缺失率  
reducing, 493 –494:降低  
miss rate vs. cache parameters, 493–494 :缺失率与缓存参数  
replacement policy, 490–491:更换策略  
status bits:状态位  
dirty bit (D), 494：脏位  
use bit (U), 490:使用位  
valid bit (V), 484 :有效位  
write policy, 494 –495 :写入策略  
write-back, 494 –495 ：回写  
write-through, 494 –495 ：透写  
CAD. See Computer-aided design:计算机辅助设计  
Callee-saved registers, 329:被调用函数保存的寄存器  
Canonical form. See Sum-of-products, Product-of-sums: 范式，另见与或式、或与式  
Capacitors, 28:电容  
Capacity, of cache, 480–481:缓存容量  
Capacity miss, 493:容量缺失  
Carry propagate adder (CPA).SeeRipple-carry adder, Carry-lookahed adder, and Prefix adder:进位传播加法器，另见行波进位加法器、先行进位加法器、前缀加法器  
Carry-lookahead adder (CLA), 241 –243, 242 :先行进位加法器  
Case statement, in HDL, 201–203.See also Switch/case statement: case语句，另见switch/case语句  
Casez, case?, in HDL, 205casez、case?语句  
Cathode, 27:阴极  
Cathode ray tube (CRT), 541–542. See also VGA monitor:阴极射线管，另见VGA显示器  
horizontal blanking interval, 542:水平消隐间隔  
vertical blanking interval, 542:垂直消隐间隔  
Cause register, 343–344, 441:cause寄存器  
Character LCDs, 538 –541字符LCD  
Characters (char), 322–324, 630, 649 :字符  
arrays, 322 –324. See also Strings数组，另见字符串  
C type, 649 :C类型  
Chips, 28 :芯片  
multiprocessors, 456:多处理器  
Chopper constant current drive, 556：斩波恒流驱动  
Circuits;电路  
74xx series. See 74xx series logic：74xx系列，另见74xx系列逻辑电路  
application-specific integrated(ASICs), 591:专用集成电路  
astable, 119:非稳态  
asynchronous, 120, 122 –123:异步  
combinational. See Combinational logic:组合，另见组合逻辑  
definition of, 55 :定义  
delay, 88 –92 :延迟  
multiple-output, 68:多路输出  
priority, 68 :优先权  
sequential. See Sequential logic:时序，另见时序电路  
synchronous, 122 –123:同步  
synchronous sequential, 120 –123, 122 ：同步时序电路  
synthesized, 176, 179, 181：综合  
timing, 88 –95:时序  
with two-stage pipeline, 160 :两级流水线  
without glitch, 95:无毛刺  
CISC. See Complex Instruction Set Computer:复杂指令集计算机  
CLBs. See Configurable logic blocks:可配置逻辑块  
Clock cycles per instruction (CPI), 444, 446 :每条指令的时钟周期  
Clock period, 142, 376:时钟周期  
Clock skew, 148 –151:时钟偏斜  
Clustered multiprocessing, 456:集群多处理  
CMOS. See Complementary MetalOxide-Semiconductor Logic:CMOS  
Combinational composition, 56 :组合构建  
Combinational logic, 174 :组合逻辑  
design, 55 –106 :设计  
Boolean algebra, 60 –66:布尔代数  
Boolean equations, 58 –60:布尔等式  
building blocks, 83 –88, 239 –254:构造部件  
delays, 88 –92 :延时  
don’t cares, 81 –82无关项  
Karnaugh maps (K-maps), 75 –83:卡诺图  
 multilevel, 66 –73：多层  
 precedence, 58：优先级  
 timing, 88 –95：时序  
 two-level, 69：两层  
 X’s (contention). See Contention：X(竞争)  
 X’s (don’t cares). See Don’t cares (X)：X(无关项)  
 Z’s (floating). See Floating (Z)：Z(悬空)  
 HDLs and. See Hardware description languages：硬件描述语言  
 truth tables with don’t cares, 69, 81 –82, 205  
Combining theorem, 62:合并律  
Command line arguments, 666–667:命令行参数  
Comments注释

in C, 627 : C语言

in MIPS assembly, 297在MIPS汇编语言

in SystemVerilog, 180在SystemVerilog语言

in VHDL, 180在VHDL语言  
Common mistakes in C, 667 –671 :C语言常见错误  
Comparators, 246 –248:比较器  
Comparison比较

in hardware. See Comparators, ALU 在硬件，另见比较器、ALU

in MIPS assembly, 319–320, 345在MIPS汇编语言

using ALU, 250使用ALU  
Compilation, in C, 626 –627, 665 –666:C语言编译  
Compiler, 338 –339:编译器  
for C, 626 –627, 665 –666: C语言  
Complementary Metal-OxideSemiconductor Logic (CMOS), 26 –34：CMOS  
Complements theorem, 62:互补定理  
Complex instruction set computer (CISC), 298, 347:复杂指令集计算机  
Complexity management, 4 –7:复杂度管理  
digital abstraction, 4 –5:数字抽象  
discipline, 5 –6:约束  
hierarchy, 6–7:层次化  
modularity, 6–7:模块化  
regularity, 6–7:规整化  
Compulsory miss, 493:强制缺失  
Computer Architecture (Hennessy &Patterson), 444:计算机体系结构  
Computer-aided design (CAD), 71, 129:计算机辅助设计  
Concurrent signal assignment statement, 179, 183–184, 193, 200–206:并行信号赋值语句  
Condition codes. See Status flags状态码，另见状态标签

Conditional assignment, 181 –182:条件赋值  
Conditional branches, 314 –315:条件分支  
Conditional operator, 181–182:条件运算符  
Conditional signal assignments,181–182:条件信号赋值  
Conditional statements条件语句

in C, 639 –640:在C语言中

if, 639–640

if/else, 639

switch/case, 639–640

in HDL, 194, 201 –205在HDL中

case, 201 –203

casez, case?, 205

if, if/else, 202 –205

in MIPS assembly, 316 –317 在MIPS汇编中

if, 316 –317

if/else, 317

switch/case, 317  
Configurable logic blocks (CLBs), 274, 589. See also Logic elements:可配置逻辑块，另见逻辑元素  
Conflict miss, 493:冲突缺失  
Consensus theorem, 62, 64:一致律  
Constants常数

in C, 627–628 :在C中

in MIPS assembly, 304, 313. See also Immediates在MIPS汇编中，另见立即数  
Contamination delay, 88 –92. See also Short path :最小延迟，另见最短路径  
Contention (X), 73–74 竞争  
Context switching, 455:上下文切换  
Continuous assignment statements, 179, 193, 200, 206 :连续赋值语句  
Control hazards, 415, 421 –424 :控制相关  
Control signals, 91, 249:控制信号  
Control unit. See also ALU decoder, :控制单元，另见ALU译码器  
Main decoder :主解码器  
of multicycle MIPS processor, 396 –408:多周期MIPS处理器  
of pipelined MIPS processor, 413 –414 :流水线MIPS处理器  
of single-cycle MIPS processor, 382 –387 :单周期MIPS处理器  
Control-flow statements:控制流语句  
conditional statements. See Conditional statements:条件语句  
loops. See Loops:循环  
Coprocessor 0 registers, 441. See also Cause and EPC协处理器0寄存器  
Core Duo microprocessor chip, 464:酷睿双核微处理器芯片  
Core i7 microprocessor chip, 465 :酷睿i7微处理器芯片  
Cores, 456 :核  
Counters, 260 :计数器  
divide-by-3, 130 :除以3  
Covering theorem, 62:吸收律  
CPA. See Carry propagate adder (CPA) :进位传播加法器  
CPI. See Clock cycles per instruction, Cycles per instruction:每条指令的时钟周期  
Critical path, 89–92, 388:最长路径  
Cross-coupled inverters, 109, 110:交叉耦合反相器  
bistable operation of, 110:双稳态运作  
CRT. See Cathode ray tube:阴极射线管  
Cycle time. See Clock period:周期时间，另见时钟周期  
Cycles per instruction (CPI), 375:每条指令的时钟周期  
Cyclic paths, 1 20:回路  
Cyclone IV FPGA, 274 –279：Cyclone IV现场可编程逻辑门阵列