D  
D flip-flops. See flip-flops: D 触发器  
D latch. See Latch : D锁存器  
D/A conversion, 533 –537 :D / A转换  
DACs. See Digital-to-analog converters:数字模拟转换器  
Data Acquisition Systems (DAQs), 562 –563:数据采集系统  
 myDAQ, 563  
Data hazards, 415 –421:数据冲突  
Data memory, 373:数据存储  
 HDL for, 439 :硬件描述语言  
Data segment, 340:数据段  
Data sheets, 591 –596:数据手册

Data types, 643 –657:数据类型

arrays. See Arrays：数组

characters. See Character (char) ：字符

dynamic memory allocation. See Dynamic memory allocation (malloc and free)：动态内存分配  
 linked list. See Linked list：链表  
 pointers. See Pointers:指针  
 strings. See Strings (str) :字符串  
 structures. See Structures (struct) :结构  
 typedef, 653 –654：typedef  
Datapath:数据通路  
 multicycle MIPS processor, 390 –396:多周期MIPS处理器  
 pipelined MIPS processor, 412 –413:流水线MIPS处理器  
 single-cycle MIPS processor, 376 –382 :单周期MIPS处理器  
DC. See Direct current :直流电  
DC motors, 548–552, 549 :直流电机  
 H-bridge, 549, 550 :H桥  
 shaft encoder, 549 –552:轴角编码器  
DC transfer characteristics, 24–26. See also Noise margins :直流传输特性  
DDR3. See Double-data rate memory:DDR3  
DE-9 cable, 524: DE-9缓存  
De Morgan’s theorem, 63:德·摩根定理  
Decimal numbers, 9:十进制数  
Decimal to binary conversion, 11:十进制-二进制转换  
Decimal to hexadecimal conversion, 13:十进制-十六进制转换  
Decode stage, 409–411:解码阶段  
Decoders :解码器  
 definition of, 86–87 :定义  
 HDL for :硬件描述语言  
 behavioral, 202–203 :行为  
 parameterized, 219 :参数化  
 logic using, 87 –88 :逻辑使用  
 Seven-segment. See Seven-segment display decoder:七段显示译码器  
Deep pipelines, 444 –445 :深度流水线  
Delay generation using counters, 528 –529:使用计数器产生延迟  
Delaymicros function, 528: Delaymicros函数  
Delays, logic gates. See Propagation delay 延时

in HDL (simulation only), 188–189 在HDL中  
DeleteUser function, 655：DeleteUser函数  
De Morgan, Augustus, 63   
De Morgan’s theorem, 63–64德·摩根定理  
Dennard, Robert, 266   
Destination register (rd or rt), 378–379, 385, 393目的地寄存器  
Device driver, 507 –508, 526设备驱动程序  
Device under test (DUT), 220测试设备  
Dice, 28切块  
Dielectric, 28电介质  
Digital abstraction, 4 –5, 7 –9, 22 –26数字抽象  
Digital circuits. See Logic数字电路  
Digital signal processor (DSP), 457 数字信号处理  
Digital system implementation, 583 –617数字系统实现  
 74xx series logic. See 74xx series logic :74xx系列逻辑电路  
 application-specific integrated circuits (ASICs), 591专用集成电路  
 assembly of, 599 –602 汇编语言  
 breadboards, 600 –601电路试验板  
 data sheets, 591 –596数据手册  
 economics, 615 –617经济学  
 logic families, 597 –599逻辑电路系列  
 packaging, 599 –602封装  
 printed circuit boards, 601 –602印刷电路板  
 programmable logic, 584 –591可编程逻辑  
Digital-to-analog converters (DACs), 531数字模拟转换器  
DIMM. See Dual inline memory module双列直插内存模块  
Diodes, 27–28二极管  
 p-n junction, 28 p-n接面  
DIPs. See Dual-inline packages 双列直插式封装

Direct current (DC) transfer characteristics, 24, 25直流电(DC)传输特性  
Direct mapped cache, 482 –486, 484直接映射缓存  
Direct voltage drive, 554直流电压驱动  
Dirty bit (D), 494重写标志位  
Discipline 约束

dynamic, 142 –151. See also Timing analysis：动态，另见时序分析

static, 142 –151. See also Noise margins：静态，另见噪声容限  
Discrete-valued variables, 7 离散数值变量  
Distributivity theorem, 63分配律  
div, 314：div  
Divide-by-3 counter 除以3计数器  
 design of, 129–131: 设计  
 HDL for, 210–211：HDL  
Divider, 253–254 除法器  
Division 除法  
 circuits, 253–254 电路  
 MIPS instruction, 314：MIPS指令  
 MIPS signed and unsigned instructions, 345：MIPS有符号与无符号指令  
divu, 345：divu  
Don’t care (X), 69, 81–83, 205: 无关项  
Dopant atoms, 27掺杂原子  
Double, C type, 630 –631：浮点数  
Double-data rate memory (DDR), 266, 561双数据速率内存  
Double-precision formats, 257 –258双精度格式  
Do/while loops, in C, 641 –642 :do/while 循环  
DRAM. See Dynamic random access memory动态随机存储器  
Dual inline memory module (DIMM), 561双列直插内存模块  
Dual-inline packages (DIPs), 28, 583, 599双列直插式封装  
Dynamic branch predictors, 446动态分支预测  
Dynamic data segment, 337动态数据段  
Dynamic discipline, 142–151. See also Timing analysis动态约束，另见时序分析  
Dynamic memory allocation (malloc, free) , 654 –655动态内存分配  
 in MIPS memory map, 337：在MIPS内存映射中  
Dynamic power, 34动态功耗  
Dynamic random access memory (DRAM), 266, 267, 475 –478, 561动态随机存储器  
  
E  
Economics, 615 经济  
Edge-triggered flip-flop. See flip-flop边沿触发触发器  
EEPROM. See Electrically erasable programmable read only memory电可擦除可编程只读存储器  
EFLAGS register, 350 ：EFLAGS寄存器  
Electrically erasable programmable read only memory (EEPROM), 269电可擦除可编程只读存储器  
Embedded I/O (input/output) systems, 508 –558 嵌入式I/O (输入/输出) 系统  
 analog I/O, 531 –537 模拟I/O  
 A/D conversion, 532 –533模/数转换  
 D/A conversion, 533 –536数/模转换  
 digital I/O, 513 –515数字I/O  
 general-purpose I/O (GPIO), 513 –515通用I/O  
 interrupts, 529 –531 中断  
 LCDs. See Liquid Crystal Displays 液晶显示屏  
 microcontroller peripherals, 537–558单片机外围设备  
 motors. See Motors 电机  
 PIC32 microcontroller, 509 –513：PIC32单片机  
 serial I/O, 515 –527. See also Serial I/O：串行I/O  
 timers, 527 –529 计时器  
 VGA monitor. See VGA monitor, 493 VGA显示器  
Enabled flip-flops, 115 –116 使能触发器  
Enabled registers, 196 –197. See also flip-flops 使能寄存器  
EPC. See Exception program counter异常程序计数器  
EPROM. See Erasable programmable read only memory可擦除可编程只读存储器

Equality comparator, 247 相等比较器  
Equation minimization 等式最简化  
 using Boolean algebra, 65–66 使用布尔代数  
 using Karnaugh maps. See Karnaug maps 使用卡诺图  
Erasable programmable read only memory (EPROM), 269, 588 可擦除可编程只读存储器  
Ethernet, 561 以太网  
Exception program counter (EPC), 343–344 异常程序计数器  
Exceptions, 343–344, 440–443 异常  
 Cause. See Cause register cause codes, 344: cause  
 EPC. See Exception program counter handler, 343 异常程序计数器处理程序  
 processor support for, 440–443 处理器支持  
 circuits, 441–442 电路  
 controller, 442–443 控制器  
Executable file, 340 可执行文件  
Execution time, 375 执行时间  
exit, 663：exit  
Extended instruction pointer (EIP), 348 扩展指令指针

F  
Factorial function call, 330–331 阶乘函数调用  
 stack during, 331 在栈  
Factoring state machines, 134–136 分解状态机  
FDIV. See Floating-point division 浮点数除法  
Field programmable gate arrays (FPGAs), 274–279, 457, 520, 543, 564, 589–591 现场可编程逻辑门阵列  
 driving VGA cable, 543 驱动VGA线  
 in SPI interface, 519–521 在SPI接口  
File manipulation, in C, 660–662 C语言中文件操作  
Finite state machines (FSMs), 123–141, 209–213 有限状态机（FSM）  
 deriving from circuit, 137–140 源于电路  
 divide-by-3 FSM, 129–131, 210–211 除以3FSM  
 factoring, 134–136, 136 分解  
 in HDL, 209–213 在HDL中  
 LE configuration for, 277–278 LE配置  
 Mealy FSM, 132–134 Mealy FSM  
 Moore FSM, 132–134 Moore FSM  
 multicycle control, 396–408, 405, 408 多周期控制  
 snail/pattern recognizer FSM, 132–134, 212–213 蜗牛/模式识别FSM  
 state encodings, 129–131. See also Binary encoding, One-cold encoding, One-hot encoding 状态编码，另见二进制编码、独冷编码、独热编码  
 state transition diagram, 124, 125 状态转换图  
 traffic light FSM, 123–129 交通灯FSM  
Fixed-point numbers, 255–256 定点数  
Flags, 250 标志  
Flash memory, 269. See also Solid state drives 闪存，另见固态硬盘  
Flip-flops, 114–118, 193–197. See also Registers 触发器，另见寄存器  
 back-to-back, 145, 152–157, 197. See also Synchronizer 背靠背，另见同步器  
 comparison with latches, 118 与锁存器比较  
 enabled, 115–116 使能  
 HDL for, 436. See also Registers: HDL，另见寄存器

metastable state of. See Metastability register, 114–115 亚稳态，另见亚稳态寄存器  
 resettable, 116 可重置  
 scannable, 262–263 可扫描  
 shift register, 261–263移位寄存器  
 transistor count, 114, 117 晶体管计数  
 transistor-level, 116–117 晶体管级  
Float, C type, 628–631 C语言浮点数  
 print formats of, 658–659 打印格式  
Floating output node, 117 浮点输出节点  
Floating point division (FDIV) bug, 175 浮点数除法错误  
Floating (Z), 74–75 浮空（Z）  
 in HDLs, 186–188 在HDL中  
Floating-gate transistor, 269. See also Flash memory 浮栅晶体管，另见闪存  
Floating-point coprocessors, 457 浮点数协处理器  
Floating-point division (FDIV), 259 浮点数除法  
Floating-point instructions, MIPS, 346–347 MIPS浮点数指令  
Floating-point numbers, 256–257 浮点数  
 addition, 258–259 加法  
 formats, single- and double-precision, 256–258 格式，单精度与双精度  
 in programming. See Float and Double 在编程中  
 rounding, 258 四舍五入  
 special cases 特殊情况  
 infinity, 257 无穷大  
 NaN, 257：NaN  
Floating-point unit (FPU), 259, 461 浮点数单元  
For loops, 319–320, 322, 642: for循环  
Format conversion (atoi, atol, atof), 663–664 格式转换(atoi, atol, atof)  
Forwarding, 416–418. See also Hazards 重定向，另见冲突

FPGAs. See Field programmable gate arrays 现场可编程逻辑门阵列  
FPU. See Floating-point unit 浮点数单元

Frequency shift keying (FSK), 548 频移键控  
 and GFSK waveforms, 548：GFSK波形  
Front porch, 542 前廊  
FSK. See Frequency Shift Keying 频移键控  
FSMs. See Finite state machines 有限状态机  
Full adder, 56, 182, 184, 200, 240 全加器  
 using always/process statement, 200 使用always/process语句  
Fully associative cache, 487–488 全相联高速缓存  
Funct field, 305, 621–622: Funct域  
Function calls, 325–333, 637–638 函数调用  
 arguments, 325–326, 637 参数  
 leaf, 330 叶子  
 naming conventions, 638 命名惯例  
 nonleaf, 330 非叶子  
 preserved and non-preserved registers, 329–332 受保护与不受保护寄存器  
 prototypes, 638 原型  
 recursive, 330–332 递归  
 return, 325–326, 637 返回  
 stack, use of, 327–333. See also Stack 栈  
 with no inputs or outputs, 325, 637 无输入或输出  
Fuse-programmable ROM, 269 熔丝型可编程ROM

G  
Gated time accumulation, 529 门控时间累加  
Gates 门  
 AND, 20, 22, 128 与  
 buffer, 20 缓冲  
 multiple-input, 21–22 多输入  
 NAND, 21, 31 与非  
 NOR, 21–22, 111, 128 或非  
 NOT, 20 非  
 OR, 21 或  
 transistor-level. See Transistors 晶体管级  
 XNOR, 21 同或  
 XOR, 21 异或  
General-purpose I/O (GPIO), 513 通用IO（GPIO）  
 PIC32 ports (pins) of, 515：PIC32端口（管脚）  
 switches and LEDs example, 513–514 开关与LED灯示例  
Generate signal, 241, 243 生成信号  
Genwaves function, 535：Genwaves函数  
Glitches, 92–95 毛刺  
Global data segment, 336–337 全局数据段  
Global pointer ($gp), 337 全局指针  
GPIO. See General-purpose I/O 通用IO  
Graphics accelerators, 464 图形加速器  
Graphics processing unit (GPU), 457 图形处理单元  
Gray codes, 76 格雷码  
Gray, Frank, 76  
Ground (GND), 22 接地  
 symbol for, 31 符号

H  
Half adder, 240, 240 半加器  
Hard disk, 478–479. See also Hard drive 硬盘  
Hard drive, 478–479, 496. See also Hard disk, Solid state drive, and Virtual memory 硬盘，另见固态硬盘、虚拟内存  
Hardware description languages (HDLs). See also SystemVerilog, VHDL 硬件描述语言，另见SystemVerilog、VHDL  
 capacity, 493 容量  
 combinational logic, 174, 198 组合逻辑  
 bitwise operators, 177–179 位操作  
 blocking and nonblocking assignments, 205–209 阻塞和非阻塞赋值  
 case statements, 201–202: case语句  
 conditional assignment, 181–182 条件赋值  
 delays, 188–189 延时  
 data types, 213–217 数据类型  
 history of, 174–175 历史  
 if statements, 202–205: if语句  
 internal variables, 182–184 内部变量  
 numbers, 185 数字  
 operators and precedence, 184–185 运算符和优先级  
 reduction operators, 180–181 缩减运算符  
 modules, 173–174 模块  
 parameterized modules, 217–220 参数化模块  
 processor building blocks, 434–437 处理器构建模块  
 sequential logic, 193–198, 209–213 时序逻辑  
 simulation and synthesis, 175–177 仿真与综合  
 single-cycle MIPS processor, 429–440 单周期MIPS处理器  
 structural modeling, 190–193 结构建模  
 testbench, 220–224, 437–438 测试程序  
Hardware handshaking, 523 硬件握手  
Hardware reduction, 70–71. See also Equation minimization 硬件减少，另见等式最简化  
Hazard unit, 416–427 冲突单元  
Hazards. See also Hazard unit 冲突，另见冲突单元  
 control hazards, 415, 421–424 控制冲突  
 data hazards, 416–421 数据冲突  
 read after write (RAW), 415, 451 写入后读取（RAW）  
 solving 解决  
 control hazards, 421–424 控制相关  
 forwarding, 416–418 重定向  
 stalls, 418–421 阻塞  
 write after read (WAR), 451 读取后写入（WAR）  
 write after write (WAW), 451–452 写入后写入（WAW）  
H-bridge control, 550：H桥控制  
HDL. See Hardware description language, SystemVerilog, and VHDL 硬件描述语言，另见SystemVerilog、VHDL  
Heap, 337 堆  
Heterogeneous multiprocessors, 456–458 异构多处理器  
Hexadecimal numbers, 11–13 十六进制数  
Hexadecimal to binary and decimal conversion, 11, 12 十六进制-二进制与十进制转换  
Hierarchy, 6 层次化  
HIGH, 22. See also 1, ON 高电平，另见1、开  
High-level programming languages, 296, 624 高级编程语言  
 compiling, assembling, and loading, 336–341 编译、汇编与载入  
 translating into assembly, 300 转换成汇编语言  
High-performance microprocessors, 444 高性能微处理器  
Hit, 478 命中  
Hit rate, 478–480 命中率  
Hold time constraint, 142–148 保持时间约束  
 with clock skew, 149–151 时钟偏移  
Hold time violations, 145, 146, 147–148, 150–151 保持时间约束违反  
Homogeneous multiprocessors, 456 同构多处理器  
Hopper, Grace, 337

I  
IA-64, 354  
IA-32 architecture. See x86：IA-32体系结构，另见x86

ICs. See Integrated circuits 集成电路

Idempotency theorem, 62 重叠定理  
Identity theorem, 62 同一性定理  
Idioms, 177 惯用语法  
If statements: if语句  
 in C, 639：C语言中  
 in HDL, 202–205：HDL中  
 in MIPS assembly, 316–317：MIPS汇编语言中  
If/else statements, 317, 649：if/else语句  
 in C, 639–640：C语言中  
 in HDL, 202–205：HDL中  
 in MIPS assembly, 317：MIPS汇编语言中  
IM. See Instruction memory 指令存储器

Immediate addressing, 333 直接寻址  
Immediates, 304, 313. See also Constants 直接数，另见常数

32-bit, 313：32位  
 immediate field, 307–308 直接数域  
 logical operations with, 311 逻辑操作  
Implicit leading one, 256 隐含前导位  
Information, amount of, 8 信息量  
Initializing 初始化  
 arrays in C, 645–646：C语言数组   
 variables in C, 633：C语言变量  
InitTimer1Interrupt function, 530：InitTimer1Interrupt函数  
Input/output elements (IOEs), 274 输入/输出元素  
Input/Output (I/O) systems, 506–569 输入/输出系统  
 device driver, 507–508, 526 设备驱动程序  
 embedded I/O systems. See Embedded I/O systems 嵌入式输入/输出系统  
 I/O registers, 507–508 I/O寄存器  
 memory-mapped I/O, 507–508 内存映射I/O  
 personal computer I/O systems. See Personal computer I/O systems 个人电脑I/O系统  
Institute of Electrical and Electronics Engineers (IEEE), 257 电气电子工程师学会  
Instruction encoding, x86, 352–354, 353 : x86指令编码  
Instruction formats, MIPS：MIPS指令格式  
 F-type, 346：F型  
 I-type, 307–308：I型  
 J-type, 308：J型  
 R-type, 305–306：R型  
Instruction formats, x86, 352–354: x86指令格式  
Instruction level parallelism (ILP), 452, 455 指令级并行  
Instruction memory (IM), 373, 411 指令存储器  
 MIPS, 440  
Instruction register (IR), 391, 398 指令存储器  
Instruction set, 295, 371–372. See also Architecture 指令集，另见体系结构  
Instructions, MIPS, 295–347, 619–622: MIPS指令  
 arithmetic, 299–300, 304, 314，344–345, 620–622 算术  
 branching, 314–316 分支  
 floating-point, 346–347, 622 浮点数  
 for accessing memory. See Loads, Stores 访问内存，另见加载、存储  
 F-type, 346：F型  
 I-type, 307–308：I型  
 J-type, 308：J型  
 logical, 308, 310–313逻辑  
 multiplication and division, 314, 345乘法和除法  
 R-type, 305–306, 621–622：R型  
 set less than, 319–320, 345 小于设置  
 signed and unsigned, 344–345 有符号和无符号  
Instructions, x86, 347–355：x86指令  
Instructions per cycle (IPC), 375 每周期指令数  
Integer Execution Unit (IEU), 461 整数执行单元  
Integrated circuits (ICs), 599 集成电路  
Intel. See x86  
Intel x86. See x86  
Interrupt service routine (ISR), 529. See also Exceptions 中断服务程序，另见异常  
Interrupts, 343, 529–531 中断  
PIC32, 529–531  
Invalid logic level, 186 无效逻辑电平  
Inverters, 20, 119, 178. See also NOT gate 反相器，另见非门

cross-coupled, 109, 110 交叉耦合  
 in HDL, 178, 199 在HDL中  
An Investigation of the Laws of Thought (Boole), 8  
Involution theorem, 62 回旋定理  
I/O. See Input/output systems 输入/输出系统  
IOEs. See Input/output elements 输入/输出元素  
IorD, 393, 397  
IPC. See Instructions per cycle 每周期指令数  
IR. See Instruction register 指令寄存器  
IRWrite, 391, 397  
ISR. See Interrupt service routine 中断服务程序

I-type instructions, 307–308: I型指令

J

j, 315–316  
jal, 325  
Java, 322. See also Language：Java语言  
jr, 315–316, 325  
JTA. See Jump target address 跳转目标地址  
J-type instructions, 308：J型指令  
Jump, MIPS instruction, 315–316：MIPS指令跳转  
Jump, processor implementation, 386–387, 404–408 跳转，处理器实现  
Jump target address (JTA), 334–335, 386 跳转目标地址

K  
Karnaugh maps (K-maps), 75–84, 93–95, 126 卡诺图  
 logic minimization using, 77–83 用于逻辑最简化  
 prime implicants, 65, 77–81, 94–95 主蕴含式  
 seven-segment display decoder, 79–81 七段显示译码器  
 with “don’t cares,” 81–82 包含无关项  
 without glitches, 95 无毛刺  
Karnaugh, Maurice, 75  
Kilobit (Kb/Kbit), 14：Kb  
Kilobyte (KB), 14：KB  
K-maps. See Karnaugh maps 卡诺图

L  
LAB. See Logic array block逻辑阵列块  
Land grid array, 558 栅格阵列  
Language. See also Instructions 编程语言，另见指令  
 assembly, 296–304 汇编  
 machine, 305–310 机器  
 mnemonic, 297 助记符  
 translating assembly to machine, 306 转换汇编语言为机器语言  
Last-in-first-out (LIFO) queue, 327. 后进先出队列  
 See also Stack 另见栈  
Latches, 111–113 锁存器  
 comparison with flip-flops, 109, 118 与触发器比较  
 D, 113, 120  
 SR, 111–113, 112  
 transistor-level, 116–117 晶体管级  
Latency, 157–160, 409–411, 418 延时  
Lattice, silicon, 27 晶格  
lb, load byte. See Loads  
lbu, load byte unsigned. See Loads  
LCDs. See Liquid crystal displays   
Leaf function, 330 叶子函数  
Leakage current, 34 泄漏电流  
Least recently used (LRU) replacement, 490–491 最近最少使用替换  
 two-way associative cache with, 490–491, 491 两路相联高速缓存  
Least significant bit (lsb), 13, 14 最低有效位  
Least significant byte (LSB), 13, 14, 302 最低有效字节  
LEs. See Logic elements 逻辑元素  
Level-sensitive latch. See D latch 电平敏感锁存器  
lh, load half. See Loads  
lhu, load half unsigned. See Loads  
LIFO. See Last-in-first-out queue 后进先出队列  
Line options, compiler and command, 665–667 编译器命令行选项  
Linked list, 655–656 链表  
Linker, 340–341 链接  
Liquid crystal displays (LCDs), 538–541液晶显示屏  
Literal, 58, 96 项  
Little-endian memory, 302–303, 302 小端存储  
Little-endian bus order in HDL, 178小端总线顺序  
Loads, 345 加载  
 base addressing of, 333 基址寻址  
 load byte (lb or lbu), 304, 323–324, 345  
 load half (lh or lhu), 345  
 load word (lw), 301–304  
Local variables, 332–333 局部变量  
Locality, 476 局部性  
Logic 逻辑  
 bubble pushing, 71–73 推气泡  
 combinational. See Combinational logic 组合逻辑  
 families, 597–599 系列  
 gates. See Gates 门  
 hardware reduction. See Equation simplification and Hardware reduction 硬件减少，另见等式化简  
 multilevel. See Multilevel combinational logic 多级，另见多级组合逻辑  
 programmable, 584–591 可编程  
 sequential. See Sequential logic 时序逻辑  
 transistor-level. See Transistors 晶体管级  
 two-level, 69 二级  
Logic array block (LAB), 275 逻辑阵列块  
Logic arrays, 272–280. See also Programmable logic arrays and Field programmable gate arrays 逻辑阵列，另见可编程逻辑阵列和现场可编程逻辑门阵列

transistor-level implementation, 279–280 晶体管级实现  
Logic elements (LEs), 274–279 逻辑元素  
 of Cyclone IV, 276  
 functions built using, 277–278 用于构建函数  
Logic families, 25, 597–599 逻辑系列  
 compatibility of, 26 兼容性  
 logic levels of, 25 逻辑电平  
 specifications, 597, 599 规范说明  
Logic gates, 19–22, 179, 584 逻辑门  
 AND. See AND gate 与门  
 AND-OR (AO) gate, 46 与或门  
 multiple-input gates, 21–22 多输入门  
 NAND. See NAND gate 与非门  
 NOR. See NOR gate 或非门  
 OR. See OR gate 或门  
 OR-AND-INVERT (OAI) gate, 46 或与非(OAI)门  
 with delays in HDL, 189 包含延时  
 XNOR. See XNOR gate 同或门  
 XOR. See XOR gate 异或门  
Logic levels, 22–23 逻辑电平  
Logic simulation, 175–176 逻辑仿真  
Logic synthesis, 176–177, 176 逻辑综合  
Logical instructions, 311–312 逻辑指令  
Logical shifter, 250 逻辑移位器  
Lookup tables (LUTs), 270, 275 查找表  
Loops, 317–319, 641–642 循环  
 in C, 在C语言中  
 do/while, 641–642  
 for, 642  
 while, 641  
 in MIPS assembly, 在MIPS汇编语言中  
 for, 319–320  
 while, 318–319  
LOW, 22. See also 0, OFF 低电平，另见0、关

Low Voltage CMOS Logic (LVCMOS), 25 低电压CMOS逻辑  
Low Voltage TTL Logic (LVTTL), 25 低电压TTL逻辑  
LRU. See Least recently used replacement 最近最少使用替换  
LSB. See Least significant byte 最低有效字节  
lsb. See Least significant bit 最低有效位  
lui, load upper immediate, 313  
LUTs. See Lookup tables 查找表  
LVCMOS. See Low Voltage CMOS Logic 低电压CMOS逻辑  
LVTTL. See Low Voltage TTL Logic 低电压TTL逻辑  
lw, load word. See Loads

M  
Machine code, assembly and, 437 机器代码，汇编语言  
Machine language, 305–310 机器语言  
 formats, 305–308 格式  
 F-type, 346：F型  
 I-type, 307–308, 307：I型  
 J-type, 308, 308：J型  
 R-type, 305–306, 305：R型  
 interpreting, 308–309 诠释  
 stored program, 309–310, 310 存储程序  
 translating assembly language to, 306 转换汇编语言为  
Magnitude comparator, 247 幅度比较器  
Main decoder, 382–387 主译码器  
 HDL for, 432  
main function in C, 625：C语言中的main函数  
Main memory, 478 主存储器  
Malloc function, 654：Malloc函数  
Mantissa, 258–259 尾数  
Mapping, 482 映射  
Master latch, 114 主锁存器  
Master-slave flip-flop, 114 主-从触发器  
Masuoka, Fujio, 269  
math.h, C library, 664–665: C语言函数库  
Max-delay constraint. See Setup time constraint 最大延时约束，另见建立时间约束  
Maxterms, 58 最大项  
MCM. See Multichip module Mealy machines, 123, 123, 132 多芯片模块Mealy机  
 state transition and output table, 134　状态转换和输出表  
 state transition diagrams, 133　状态转换图  
 timing diagrams for, 135　时序图  
Mean time between failure (MTBF), 153–154平均故障间隔时间  
Medium-scale integration (MSI) chips, 584中等规模集成（MSI）芯片  
Memory. See also Memory arrays 存储器，另见存储器阵列

　　addressing modes, 349　寻址模式  
 area and delay, 266–267　面积和延迟  
 arrays. See Memory arrays average memory access time, 479　阵列，另见存储器阵列平均内存访问时间  
 big-endian, 178, 302–303　大端  
 byte-addressable, 301–303　字节可寻址  
 HDL for, 270–272  
 hierarchy, 478　层次  
 little-endian, 178, 302–303　小端  
 logic using, 270–272　逻辑  
 main, 478　主  
 operands in, 301–304　操作数  
 physical, 497　物理  
 ports, 265　端口  
 protection, 503. See also Virtual memory　保护，另见虚拟内存  
 types, 265–270　类型  
 DDR, 267  
 DRAM, 266  
 flash, 269–270　闪存  
 register file, 267–268　寄存器文件  
 ROM, 268–270  
 SRAM, 266  
　　virtual, 478. See also Virtual memory　虚拟内存  
Memory arrays, 263–272.See also Memory 存储器阵列，另见存储器  
 bit cell, 264–269 位元  
 HDL for, 270–272  
 logic using, 270–272 逻辑  
 organization, 263–265 组成  
Memory hierarchy, 478–479 存储器层次  
Memory interface, 475–476 存储器接口  
Memory map 内存映射  
 MIPS, 336–337, 341, 507  
 PIC32, 509–510  
Memory Performance. See Average Memory Access Time 存储器性能，另见平均内存访问时间  
Memory protection, 503 存储器保护  
Memory systems, 475 存储器系统  
 MIPS, 495  
 performance analysis, 479–480 性能分析  
 x86, 564–568  
Memory-mapped I/O 内存映射I/O  
 address decoder, 507 地址译码器  
 communicating with I/O devices, 507–508 与I/O设备通信  
 hardware, 508 硬件  
Mem Write, 379, 397  
MemtoReg, 380, 397  
Metal-oxide-semiconductor field effect transistors (MOSFETs), 26 金属氧化物半导体场效应晶体管  
 switch models of, 30 开关模型  
Metastability, 151–157 亚稳态  
 metastable state, 110, 151 亚稳态  
 resolution time, 151–152, 154–157 解析时间  
 synchronizers, 152–154 同步器  
mfc0. See Move from coprocessor 0  
Microarchitecture, 351–466. See also Architecture 微结构，另见体系结构  
 advanced. See Advanced microarchitecture 先进微结构  
 architectural state. See Architectural state 架构状态  
 description of, 371–374 描述  
 design process, 372–374 设计流程  
 HDL representation, 429–440: HDL表示  
 multicycle processor. See Multicycle MIPS processor 多周期处理器，另见多周期MIPS处理器  
 performance analysis, 374–376. See also Performance analysis 性能分析  
 pipelined processor. See Pipelined MIPS processor 流水线处理器，另见流水线MIPS处理器  
 single-cycle processor. See Single-cycle MIPS processor单周期处理器，另见单周期MIPS处理器  
 x86, 458–465  
 evolution of, 458 演化  
Microchip ICD3, 513  
Microchip In Circuit Debugger 3  
 (ICD3), 513  
Microcontroller, 508 微控制器  
 PIC32 (PIC32MX675F512H), 509–513, 510  
 64-pin TQFP package in, 511：64管脚TQFP封装  
 operational schematic of, 512 运作原理图  
 to PC serial link, 526 到PC串行链路  
 pinout of, 511引脚  
 virtual memory map of, 510 虚拟内存映射  
Microcontroller peripherals, 537–558 微控制器外围设备  
 Bluetooth wireless communication, 547–548 蓝牙无线通信  
 character LCD, 538–541 字符LCD  
 control, 540–541 控制  
 parallel interface, 539 并行接口  
 motor control, 548–549 电机控制  
 VGA monitor, 541–547: VGA显示器  
Microcontroller units (MCUs), 508 微控制器单元  
Micro-ops, 461 微操作  
Microprocessors, 3, 13, 295 微处理器  
 architectural state of, 310 架构状态  
 designers, 444 设计者  
 high-performance, 444 高性能  
Millions of instructions per second, 409 每秒百万指令  
Min-delay constraint. See Hold time constraint 最小延时约束，另见保持时间约束  
Minterms, 58 最小项  
MIPS. See also Architecture and Microarchitecture: MIPS，另见体系结构和微结构  
 architecture, 296, 509 体系结构  
 floating-point instructions, 346, 346–347 浮点数指令  
 instruction set, 385 指令集  
 microarchitectures 微结构  
 multicycle. See Multicycle MIPS processor 多周期，另见多周期MIPS处理器  
 pipelined. See Pipelined MIPS processor 流水线，另见流水线MIPS处理器  
 single-cycle. See Single-cycle MIPS processor 单周期，另见单周期MIPS处理器  
 microprocessor, 441, 452, 455 微处理器  
 data memory, 373 数据存储器  
 instruction memory, 373 指令存储器  
 program counter, 373 程序存储器  
 register file, 373 寄存器文件  
 state elements of, 373 状态元素  
 processor control, 344 处理器控制  
 register set, 300 寄存器集  
 vs. x86 architecture, 348 跟x86体系结构比较  
MIPS instructions, 295–356, 219–222：MIPS指令  
 branching. See Branching 分支

formats 格式  
 F-type, 622：F型  
 I-type, 307, 307–308：I型  
 J-type, 308, 308：J型  
 R-type, 305–307：R型  
 multiplication and division, 314, 345 乘法和除法  
 opcodes, 620–621 操作码  
 R-type funct fields, 621–622: R型funct域  
MIPS processors. See MIPS multi-cycle processor, MIPS pipelined processor, and MIPS single-cycle processor: MIPS处理器，另见MIPS多周期处理器、MIPS流水线处理器和MIPS单周期处理器  
 HDL for. See MIPS single-cycle HDL：HDL，另见MIPS单周期HDL  
MIPS registers, : MIPS寄存器  
 co-processor 0 registers, 344, 441–443 协处理器0寄存器  
 program counter, 310, 372–373 程序计数器  
 register file, 372–373 寄存器文件  
 register set, 298–300 寄存器集  
MIPS single-cycle HDL, 429–440: MIPS单周期HDL  
 building blocks, 434–437 构建模块  
 controller, 429 控制器  
 datapath, 429 数据通路  
 testbench, 437–440 测试程序  
Miss, 478–480, 493 缺失  
 capacity, 493 容量  
 compulsory, 493 强制  
 conflict, 486, 493 冲突  
Miss penalty, 488 缺失惩罚  
Miss rate, 478–480 缺失率  
 and access times, 480 访问次数  
Misses 缺失  
 cache, 478 缓存  
 capacity, 493 容量  
 compulsory, 493 强制  
 conflict, 493 冲突  
 page fault, 497 页面失效  
Modularity, 6 模块化  
Modules, in HDL behavioral and structural, 173–174 模块，在HDL行为模型和结构模型  
 parameterized modules, 217–220 参数化模块  
Moore, Gordon, 30  
Moore machines, 123, 132: Moore机  
 state transition and output table, 134 状态转换和输出表  
 state transition diagrams, 133 状态转换图  
 timing diagrams for, 135 时序图

Moore’s law, 30 摩尔定律  
MOS transistors. See Metal-oxide semiconductor field effect transistors 金属氧化物半导体场效应晶体管  
MOSFET. See Metal-oxide semiconductor field effect transistors 金属氧化物半导体场效应晶体管  
Most significant bit (msb), 13, 14 最高有效位  
Most significant byte (MSB), 13, 14, 302 最高有效字节  
Motors 电机  
 DC, 548–552 直流  
 H-bridge, 550：H桥  
 servo, 549, 552–554 伺服  
 stepper, 548, 554–558 步进  
Move from coprocessor 0 (mfc0), 344, 441–443. See also Exceptions: mfc0，另见异常  
MPSSE. See Multi-Protocol Synchronous Serial Engine 多协议同步串行引擎  
MSB. See Most significant byte 最高有效字节  
msb. See Most significant bit 最高有效位  
MSI chips. See Medium-scale integration 中等规模集成  
MTBF. See Mean time between failure 平均故障间隔时间  
mul, multiply, 32-bit result, 314  
mult, multiply, 64-bit result, 314  
Multichip module (MCM), 566 多芯片模块  
Multicycle MIPS processor, 389–408 多周期MIPS处理器  
 control, 396–404 控制  
 datapath, 390–396 数据通路  
 performance, 405–408 性能  
Multilevel combinational logic, 69–73. See also Logic 多级组合逻辑，另见逻辑  
Multilevel page tables, 504–506 多级页表  
Multiple-output circuit, 68–69 多输出电路  
Multiplexers, 83–86 多路选择器  
 definition of, 83–84 定义  
 HDL for：HDL  
 behavioral model of, 181–183 行为模型  
 parameterized N-bit, 218–219 参数化N位  
 structural model of, 190–193 结构模型  
 logic using, 84–86 逻辑  
 symbol and truth table, 83 符号和真值表  
Multiplicand, 252 被乘数  
Multiplication, 314, 345. See also Multiplier 乘法，另见乘法器  
 MIPS instruction, 314：MIPS指令  
 signed and unsigned instructions, 345 有符号和无符号指令  
Multiplier, 252–253 乘法器  
 schematic, 252 电路图  
 HDL for, 253: HDL  
Multiprocessors 多处理器  
 chip, 456 芯片  
 heterogeneous, 456–458 异构  
 homogeneous, 456 同构  
Multi-Protocol Synchronous Serial Engine (MPSSE), 563, 563 多协议同步串行引擎  
Multithreaded processor, 455 多线程处理器  
Multithreading, 455多线程  
multu, 345  
Mux. See Multiplexers 多路选择器  
myDAQ, 563

N  
NAND (7400), 585 与非（7400）  
NAND gate, 21, 21, 31 与非门  
 CMOS, 31–32, 31–32  
Nested if/else statement, 640 嵌套if/else语句  
Nibbles, 13–14 半字节  
nMOS transistors, 28–31, 29–30：nMOS晶体管  
Noise margins, 23–26, 23 噪声容限  
 calculating, 23–24 计算  
Nonarchitectural state, 372 非架构状态  
Nonblocking and blocking assignments, 199–200, 205–209 非阻塞与阻塞赋值  
Nonleaf function, 330 非叶子函数  
Nonpreserved registers, 329, 330 不受保护寄存器  
nop, 342  
nor, 311  
NOR gate, 21–22, 111, 128, 585 或非门  
 chip (7402), 585 芯片  
 CMOS, 32  
 pseudo-nMOS logic, 33 伪nMOS逻辑  
 truth table, 22 真值表  
Not a number (NaN), 257：NaN  
NOT gate, 20 非门  
 chip (7404), 585 芯片  
 CMOS, 31  
Noyce, Robert, 26  
Null element theorem, 62 零元定理  
Number conversion 数字转换  
 binary to decimal, 10–11 二进制-十进制  
 binary to hexadecimal, 12 二进制-十六进制  
 decimal to binary, 11, 13 十进制-二进制  
 decimal to hexadecimal, 13 十进制-十六进制  
 hexadecimal to binary and decimal, 11, 12 十六进制-二进制和十进制  
 taking the two’s complement, 16 取2的补码  
Number systems, 9–19 数字系统  
 binary, 9–11, 10–11 二进制  
 comparison of, 18–19, 19 比较  
 decimal, 9 十进制  
 estimating powers of two, 14 估算2的次方  
 fixed-point, 255, 255–256 定点数  
 floating-point, 256–259 浮点数  
 addition, 258–259, 259 加法  
 special cases, 257 特殊情况  
 hexadecimal, 11–13, 12 十六进制  
 negative and positive, 15 负数和正数  
 signed, 15 有符号数  
 unsigned, 9–11 无符号数

O  
OFF, 23. See also 0, LOW 关，另见0、低电平  
Offset, 391, 392 偏移  
ON, 23. See also 1, HIGH 开，另见1、高电平  
One-bit dynamic branch predictor, 446–447 一位动态分支预测  
One-cold encoding, 130 独冷编码  
One-hot encoding, 129–131 独热编码  
One-time programmable (OTP), 584 一次性可编程（OTP）  
Opcode, 305, 620–621 操作码  
Operands 操作数  
 MIPS, 298–304  
 immediates (constants), 304, 313 直接数（常数）  
 memory, 301–304 存储器  
 registers, 298–300 寄存器  
 x86, 348–350, 349  
Operation code. See Opcode 操作代码，另见操作码  
Operators 运算符  
 in C, 633–636 在C语言中  
 in HDL, 177–185 在HDL中  
 bitwise, 177–181 位操作  
 precedence, 185 优先级  
 reduction, 180–181 缩减  
 table of, 185 表  
 ternary, 181–182 三元  
or, 311  
OR-AND-INVERT (OAI) gate, 46 或与非(OAI)门  
OR gate, 21 或门  
ori, 311–312  
OTP. See One-time programmable 一次性可编程  
Out-of-order execution, 453 乱序执行  
Out-of-order processor, 450–452 乱序处理器  
Overflow 溢出  
 handling exception for, 343–345, 440–443 处理异常  
 with addition, 15 加法  
Oxide, 28 氧化物

P  
Packages, chips, 599–600 封装，芯片  
Packed arithmetic, 454: 封装算术  
Page fault, 497: 页面失效  
Page number, 498: 页码  
Page offset, 498：页偏移  
Page table, 498, 500–501: 页表  
 number, 504 号码  
 offset, 504 偏移  
Pages, 497：页  
Paging, 504：分页  
Parallel I/O, 515: 并行I/O  
Parallelism, 157–160：并行  
Parity gate. See XOR：奇偶校验门，另见异或门  
Partial products, 252：部分乘积  
Pass by reference, 644: 按引用传递  
Pass by value, 644: 按数值传递  
Pass gate. See Transmission gates 传输门  
PC. See Program counter or Personal computer: 个人电脑  
PCB. See Printed circuit board: 印刷电路板  
PCI. See Peripheral Component Interconnect: 外围组件互连  
PCI express (PCIe), 560: PCIe  
PC-relative addressing, 333–334: PC相对寻址  
PCSrc, 395, 396–397, 397  
PCWrite, 393, 397  
Pentium processors, 460, 462: Pentium处理器  
 Pentium 4, 375, 463, 463–464   
 Pentium II, 461   
 Pentium III, 375, 461, 462   
 Pentium M, 464   
 Pentium Pro, 461   
Perfect induction, proving theorems using, 64–65 完全归纳法，证明定理  
Performance Analysis, 374–376. See also Average Memory Access Time：性能分析，另见平均内存访问时间  
 multi-cycle MIPS processor, 405–407：多周期MIPS处理器  
 pipelined MIPS processor, 426–428: 流水线MIPS处理器  
  processor comparison, 428: 处理器比较  
 single-cycle MIPS processor, 388–389: 单周期MIPS处理器  
Periodic interrupts, 530–531: 周期性中断  
Peripheral bus clock (PBCLK), 512：外设总线时钟  
Peripheral Component Interconnect (PCI), 560: 外围组件互连  
Peripherals devices. See Input/output systems：外围设备，另见输入/输出系统  
Personal computer (PC). See x86：个人电脑  
Personal computer (PC) I/O systems, 558–564：个人电脑I/O系统  
 data acquisition systems, 562–563: 数据采集系统  
 DDR3 memory, 561: DDR3内存  
 networking, 561–562: 联网  
 PCI, 560: 外围组件互连  
 SATA, 562：SATA   
 USB, 559–560, 563–564：USB  
Phase locked loop (PLL), 544：锁相环路  
Physical address extension, 567：物理地址扩展  
Physical memory, 497：物理内存  
Physical page number (PPN), 499: 物理页码  
Physical pages, 497: 物理页  
PIC32 microcontroller: PIC32单片机  
 (PIC32MX675F512H), 509–513. See also Embedded I/O systems：(PIC32MX675F512H)，另见嵌入式I/O系统  
Pipelined MIPS processor, 409–428：流水线MIPS处理器  
 abstract view of, 411：抽象视图  
 control, 413–414 控制  
 datapath, 412–413：数据通路  
 description, 409–412 描述  
 hazards, 414–426. See also Hazards 冲突

performance, 426–428: 性能

throughput, 411：吞吐量  
Pipelining, 158–160. See also Pipelined MIPS processor：流水线，另见流水线MIPS处理器  
PLAs. See Programmable logic arrays：可编程逻辑阵列  
Plastic leaded chip carriers (PLCCs), 599：塑封引线芯片载体  
Platters, 496 盘片  
PLCCs. See Plastic leaded chip carriers: 塑封引线芯片载体  
PLDs. See Programmable logic devices：可编程逻辑器件  
PLL. See Phase locked loop：锁相环路  
pMOS transistors, 28–31, 29：pMOS晶体管  
Pointers, 643–645, 647, 650, 652, 654 指针  
POS. See Product-of-sums form：POS，另见或与式  
Positive edge-triggered flip-flop, 114：正边沿触发触发器  
Power consumption, 34–35: 能量消耗  
Power processor element (PPE), 457: Power处理单元（PPE）  
PPN. See Physical page number：物理页码  
Prefix adders, 243–245, 244：前缀加法器  
Prefix tree, 245：前缀树  
Preserved registers, 329–330, 330: 受保护寄存器  
Prime implicants, 65, 77：主蕴含式  
Printed circuit boards (PCBs), 601–602：印刷电路板  
printf, 657–659  
Priority 优先级  
 circuit, 68–69 电路  
 encoder, 102–103, 105 编码器  
Procedure calls. See Function calls: 过程调用，另见函数调用  
Processor-memory gap, 477 处理器-存储器差距  
Processor performance comparison: 处理器性能比较  
 multicycle MIPS processor, 407–408: 多周期MIPS处理器  
 pipelined MIPS processor, 428: 流水线MIPS处理器  
 single-cycle processor, 388–389:单周期MIPS处理器  
Product-of-sums (POS) form, 60：或与式  
Program counter (PC), 310, 333, 373, 379: 程序计数器  
Programmable logic arrays (PLAs), 67, 272–274, 588–589: 可编程序逻辑阵列  
transistor-level implementation, 280: 晶体管级实现  
Programmable logic devices (PLDs), 588: 可编程逻辑器件  
Programmable read only memories (PROMs), 268, 270, 584–588: 可编程只读存储器  
Programming 编程  
 arrays. See Arrays 数组  
 branching. See Branching 分支  
 conditional statements, 316–317 条件语句  
 constants. See Constants, Immediates 常数，另见直接数  
 function calls. See Functions 函数调用，另见函数  
 in C. See C programming：C语言编程  
 in MIPS, 310–333 在MIPS中  
 instructions, 619–622 指令  
 logical instructions, 311–312 逻辑指令  
 loops. See Loops 循环  
 multiplication and division, 314 乘法和除法  
 shift instructions, 312–313, 312: 移位指令  
PROMs. See Programmable read only memories: 可编程只读存储器  
Propagate signal, 241:传播信号  
Propagation delay, 88–92. See also Critical path: 传输延迟，另见关键路径  
Pseudo-direct addressing, 334–335：伪直接寻址  
Pseudo instructions, 342–343：伪指令  
Pseudo-nMOS logic, 33–34, 33：伪nMOS逻辑  
 NOR gate, 33 或非门  
 ROMs and PLAs, 279–280：ROM和PLA  
Pulse-Width Modulation (PWM),536–537 脉宽调制(PWM)  
 analog output with, 537 模拟输出  
 duty cycle, 536 占空比  
 signal, 536 信号  
PWM. See Pulse-Width Modulation 脉宽调制

Q  
Quiescent supply current, 34：静态电源电流

R  
Race conditions, 119–120, 120: 竞争条件  
rand, 662–663  
Random access memory (RAM), 265–267, 271：随机存取存储器  
Read after write (RAW) hazards, 415, 451. See also Hazards：写入后读取(RAW)冲突  
Read only memory (ROM), 265, 268–269, 268–270：只读存储器  
 transistor-level implementation, 279–280：晶体管级实现  
ReadData, 378   
Read/write head, 496：读/写头  
Receiver gate, 22: 接收门  
Recursive function calls, 330–332: 递归函数调用  
Reduced instruction set computer (RISC), 298: 精简指令集计算机(RISC)  
Reduction operators, 180–181：缩减运算符  
RegDst, 381, 384, 397  
Register file (RF)：寄存器文件  
 HDL for, 435  
 in pipelined MIPS processor (write on falling edge), 412 在流水线MIPS处理器中（下降沿写入）  
 MIPS register descriptions, 299–30: MIPS寄存器描述  
 schematic, 267–268 电路图  
 use in MIPS processor, 373 在MIPS处理器中使用  
Register renaming, 452–454：寄存器重命名  
Register set, 299–300. See also Register file寄存器组，另见寄存器文件  
Register-only addressing, 333 寄存器寻址  
Registers. See Flip-flops, MIPS registers, and x86 registers：寄存器，另见触发器、MIPS寄存器和x86寄存器  
Regularity, 6：规整化  
RegWrite, 378, 384, 397, 413, 414  
Replacement policies, 504：替换策略  
Reserved segment, 337: 保留段  
Resettable flip-flops, 116：复位触发器  
Resettable registers, 194–196：复位寄存器  
Resolution time, 151–152：解析时间  
 derivation of, 154–157 来源  
 See also Metastability：另见亚稳态  
RF. See Register file：寄存器文件  
Ring oscillator, 119, 119：环形振荡器  
Ripple-carry adder, 240, 240–241, 243：行波进位加法器  
Rising edge, 88：上升沿  
ROM. See Read only memory: 只读存储器  
Rotations per minute (RPM), 549:每分钟转数(RPM)  
Rotators, 250–252: 旋转器  
Rounding modes, 258: 舍入模式  
RPM. See Rotations per minute: 每分钟转数  
RS-232, 523–524：RS-232  
R-type instructions, 305–306 : R型指令

S  
Sampling, 141: 采样  
Sampling rate, 531：采样率  
Sampling time, 532: 采样时间  
SATA. See Serial ATA：SATA，另见串行ATA   
sb, store byte. See Stores: sb, store byte，另见存储  
Scalar processor, 447：标量处理器  
Scan chains, 261–263：扫描链  
scanf, 660  
Scannable flip-flop, 262–263：可扫描触发器  
Schematics, rules of drawing, 31, 67：电路图，绘图规则  
SCK. See Serial Clock：串行时钟  
SDI. See Serial Data In: 串行数据输入  
SDO. See Serial Data Out: 串行数据输出  
SDRAM. See Synchronous dynamic random access memory: 同步动态随机存取存储器  
Segment descriptor, 353: 段描述符  
Segmentation, 354: 分段  
Selected signal assignment statements, 182：选择信号赋值语句  
Semiconductors, 27半导体  
 industry, sales, 3 工业，销售  
Sequencing overhead, 143–144, 149, 160, 428 测序开销  
Sequential building blocks. See Sequential logic 时序逻辑构建模块，另见时序逻辑  
Sequential logic, 109–161, 260–263：时序逻辑  
 counters, 260 计数器  
 finite state machines. See Finite state machine 有限状态机  
 flip-flops, 114–118. Also see Registers 触发器，另见寄存器  
 latches, 111–113 锁存器  
 D, 113  
 SR, 111–113  
 registers. See Registers 寄存器  
 shift registers, 261–263 移位寄存器  
 timing of. See Timing Analysis 时序，另见时序分析  
Serial ATA (SATA), 562：串行ATA  
Serial Clock (SCK), 516：串行时钟  
Serial communication, with PC, 525–527 串行通信，与PC  
Serial Data In (SDI), 516串行数据输入  
Serial Data Out (SDO), 516串行数据输出  
Serial I/O, 515–527串行I/O  
 SPI. See Serial peripheral interface: 串行外设接口  
 UART. See Universal Asynchronous Receiver Transmitter: 通用异步收发器  
Serial Peripheral Interface (SPI), 515–521: 串行外设接口  
 connection between PIC32 and FPGA, 519: PIC32与FPGA连接  
 ports 端口  
 Serial Clock (SCK), 516 串行时钟  
 Serial Data In (SDI), 516 串行数据输入  
 Serial Data Out (SDO), 516 串行数据输出  
 register fields in, 517 寄存器域  
 slave circuitry and timing, 520 从电路与时序  
 waveforms, 516 波形  
Servo motor, 549, 552–554:伺服电机  
Set bits, 483: 设置位  
set if less than immediate (slti), 345: slti  
set if less than immediate unsigned (sltiu), 345: sltiu  
set if less than (slt): slt  
 circuit, 250 电路  
 in MIPS assembly, 319–320在MIPS汇编中  
set if less than unsigned (sltu), 345：sltu  
Setup time constraint, 142, 145–147 建立时间约束  
 with clock skew, 148–150 包含时钟偏移  
Seven-segment display decoder, 79–82 七段显示译码器  
 HDL for, 201–202  
 with don’t cares, 82–83 包含无关项  
SFRs. See Special function registers 特殊功能寄存器  
sh, store half. See Stores：sh  
Shaft encoder, 552, 552: 轴角编码器  
Shift instructions, 312–313, 312: 移位指令  
Shift registers, 261–263: 移位寄存器  
Shifters, 250–252: 移位器  
Short path, 89–92: 最短路径  
Sign bit, 16: 符号位  
Sign extension, 18, 308: 符号扩展  
 HDL for, 436  
Signed and unsigned instructions, 344–345有符号和无符号指令  
Signed binary numbers, 15–19：有符号二进制数  
Signed multiplier, 217：有符号乘法器  
Sign/magnitude numbers, 15–16, 255 带符号的原码  
Silicon dioxide (SiO2), 28：二氧化硅  
Silicon lattice, 27: 硅晶格  
SIMD. See Single instruction multiple data: SIMD，另见单指令多数据  
Simple programmable logic devices (SPLDs), 274：简单可编程逻辑器件  
Simulation waveforms, 176：仿真波形  
 with delays, 189 包含延时  
Single-cycle MIPS processor, 376–389: 单周期MIPS处理器  
 control, 382–385 控制  
 datapath, 376–382 数据通路  
 example operation, 384–385 操作示例  
 HDL of, 429–440  
 performance, 389 性能  
Single instruction multiple data (SIMD), 447, 454, 463: 单指令多数据(SIMD)  
Single-precision formats, 257–258. See also Floating-point numbers：单精度格式，另见浮点数  
Skew. See Clock skew：偏斜，另见时钟偏斜  
Slash notation, 56：斜线记法  
Slave latch, 114. See also D flip-flop 从锁存器，另见D触发器  
sll, 312  
sllv, 313  
SLT. See set if less than  
slt, set if less than, 319–320  
slti, 345  
sltiu, 345  
sltu, 345  
Small-scale integration (SSI) chips, 584小规模集成芯片  
Solid state drive (SSD), 478–479. See also Flash memory and Hard drive：固态硬盘，另见闪存和硬盘  
SOP. See Sum-of-products form ：SOP，另见与或式  
Spatial locality, 476, 488–490：空间局部性  
Spatial parallelism, 157–158：空间并行  
Special function registers (SFRs), 509：特殊功能寄存器  
SPECINT2000, 406  
SPI. See Serial Peripheral Interface：串行外设接口  
Spinstepper function, 557：Spinstepper函数  
SPIxCON, 516  
Squashing, 452 挤压  
SR latches, 111–113, 112：SR锁存器  
SRAM. See Static random access memory：静态随机存取存储器  
srand, 662–663  
srl, 312  
srlv, 313  
SSI chips. See Small-scale integration小规模集成芯片  
Stack, 327–333. See also Function calls 栈，另见函数调用  
 during recursive function call, 331 在递归函数调用中  
 preserved registers, 329–330 受保护寄存器  
 stack frame, 328, 332 栈帧  
 stack pointer ($sp), 327 栈指针  
 storing additional arguments on, 332–333 存储额外参数  
 storing local variables on, 332–333 存储局部变量  
Stalls, 418–421. See also Hazards 阻塞，另见冲突  
Standard libraries, 657–665：标准程序库  
 math, 664–665  
 stdio, 657–662  
 file manipulation, 660–662 文件操作  
 printf, 657–659  
 scanf, 660  
 stdlib, 662–664  
 exit, 663  
 format conversion (atoi, atol, atof), 663–664 格式转换(atoi, atol, atof)  
 rand, srand, 662–663  
 string, 665  
State encodings, FSM, 129–131, 134. See also Binary encoding, One-cold encoding, One-hot encoding : FSM状态编码，另见二进制编码、独冷编码、独热编码  
State machine circuit. See Finite state machines：状态机电路，另见有限状态机  
State variables, 109：状态变量  
Static branch prediction, 446：静态分支预测  
Static discipline, 24–26：静态约束  
Static power, 34：静态功耗  
Static random access memory (SRAM), 266, 267: 静态随机存取存储器  
Status flags, 350: 状态标志  
stdio.h, C library, 657–662. See also Standard libraries: stdio.h，C函数库，另见标准函数库  
stdlib.h, C library, 662–664. See also Standard libraries: stdlib.h，C函数库，另见标准函数库  
Stepper motors, 549, 554–556 步进电机  
 bipolar stepper motor, 554–555 双极步进电机  
 half-step drive, 554 半步驱动  
 two-phase-on drive, 554 两相驱动  
 wave drive, 554 波驱动  
Stored program, 309–310 存储程序  
Stores 存储  
 store byte (sb or sbu), 302–304, 323–324 存储字节(sb 或 sbu),  
 store half (sh or shu), 345 存储半字(sh 或 shu)  
 store word (sw), 302–304 存储字(sw)  
string.h, C library, 665: string.h，C函数库  
Strings, 324, 650–651. See also Characters (char) 字符串，另见字符（char）  
Structural modeling, 173–174, 190–193: 结构建模  
Structures (struct), 651–653：结构(struct)  
sub, 297  
Substrate, 28–29：衬底  
Subtraction, 17, 246, 297: 减法  
 signed and unsigned instructions 344–345有符号和无符号指令  
Subtractor, 246–247: 减法器  
subu, 345  
Sum-of-products (SOP) form, 58–60 与或式  
Superscalar processor, 447–449：超标量处理器  
Supply voltage, 22. See also VDD 电源电压，另见VDD

sw, store word, 302–304. See also Stores：sw，存储字，另见存储  
Swap space, 504：交换空间  
Switch/case statements ：Switch / case语句  
 in C, 639–640在C语言中  
 in HDL. See Case statement 在HDL中，另见case语句  
 in MIPS assembly, 317 在MIPS汇编中  
Symbol table, 339符号表  
Symmetric multiprocessing (SMP). See Homogeneous multiprocessors: 对称多处理，另见同构多处理器  
Synchronizers, 152–154, 152–153: 同步器  
Synchronous circuits, 122–123: 同步电路  
Synchronous dynamic random access memory (SDRAM), 267同步动态随机存取存储器(SDRAM)  
 DDR, 267  
Synchronous logic, design, 119–123：同步逻辑设计  
Synchronous resettable flip-flops, 116：同步复位触发器  
Synchronous sequential circuits, 120–123, 122. See also Finite state machines：同步时序电路，另见有限状态机  
 timing specification. See Timing analysis：时序规范，另见时序分析  
Synergistic processor elements (SPEs), 457：协同处理器元素(SPE)  
Synergistic Processor Unit (SPU) ISA, 458：协同处理器单元(SPU) ISA  
SystemVerilog, 173–225. See also Hardware description languages: SystemVerilog，另见硬件描述语言

accessing parts of busses, 188, 192 访问总线部件  
 bad synchronizer with blocking assignments, 209 使用阻塞赋值的错误的同步器  
 bit swizzling, 188 位交叉混合  
 blocking and nonblocking assignment, 199–200, 205–208 阻塞和非阻塞赋值  
 case statements, 201–202, 205：case语句  
 combinational logic using, 177–193, 198–208, 217–220 组合逻辑  
 comments, 180 注释  
 conditional assignment, 181–182 条件语句  
 data types, 213–217 数据类型  
 decoders, 202–203, 219 译码器  
 delays (in simulation), 189 延时（在仿真中）  
 divide-by-3 FSM, 210–211 除以3 FSM  
 finite state machines (FSMs), 209–213 : 有限状态机  
 Mealy FSM, 213  
 Moore FSM, 210, 212  
 full adder, 184 全加器  
 using always/process, 200 使用always/process  
 using nonblocking assignments, 208 使用非阻塞赋值  
 history of, 175 历史  
 if statements, 202–205：if语句  
 internal signals, 182–184 内部信号  
 inverters, 178, 199 反相器  
 latches, 198 锁存器  
 logic gates, 177–179:逻辑门  
 multiplexers, 181–183, 190–193, 218–219: 多路选择器  
 multiplier, 217：乘法器  
 numbers, 185–186 数字  
 operators, 185 运算符  
 parameterized modules, 217–220：参数化模块  
 N:2N decoder, 219：N:2N 译码器  
 N-bit multiplexers, 218–219：N位多路选择器  
 N-input AND gate, 220：N输入与门  
 priority circuit, 204: 优先级电路  
 using don’t cares, 205 使用无关项  
 reduction operators, 180–181 缩减运算符  
 registers, 193–197 寄存器  
 enabled, 196 使能  
 resettable, 194–196 复位  
 sequential logic using, 193–198, 209–213 时序逻辑  
 seven-segment display decoder, 201七段显示译码器  
 simulation and synthesis, 175–177仿真和综合  
 structural models, 190–193 结构模型  
 synchronizer, 197 同步器  
 testbench, 220–224, 437–438 测试程序  
 self-checking, 222 自测试  
 simple, 221 简单  
 with test vector file, 223–224带测试向量  
 tristate buffer, 187 三态缓冲  
 truth tables with undefined and floating inputs, 187, 188 带不确定和浮空输入的真值表  
 z’s and x’s, 186–188, 205：z和x

T  
Tag, 483 标签  
Taking the two’s complement, 16–17 取2的补码  
Temporal locality, 476, 481–482, 485, 490：时间局部性  
Temporal parallelism, 158–159：时间并行  
Temporary registers, 299, 329–330：临时寄存器  
Ternary operators, 181, 635：三元运算符  
Testbenches, HDLs, 220–224 测试程序，HDL  
 for MIPS processor, 437–438：MIPS处理器  
 simple, 220–221简单  
 self-checking, 221–222自测试  
 with testvectors, 222–224带测试向量  
Text segment, 336, 340文本段  
Thin Quad Flat Pack (TQFP), 510：薄型四方扁平封装(TQFP)  
Thin small outline package (TSOP), 599：薄型小尺寸封装(TSOP)  
Thread level parallelism (TLP), 455：线程级并行  
Threshold voltage, 29：阈值电压  
Throughput, 157–160, 374–375, 409–411, 455：吞吐量  
Timers, 527–529 计时器  
 delay generation using, 528–529 延时生成

Timing 时序

of combinational logic, 88–95 组合逻辑

delay. See Propagation delay, Contamination delay 延迟，另见传输延迟、最小延迟

glitches. See Glitches 毛刺

of sequential logic, 141–157 时序逻辑

analysis. See Timing analysis 分析，另见时序分析

clock skew. See Clock skew 时钟偏移  
dynamic discipline, 141–142 动态约束

metastability. See Metastability 亚稳态

resolution time. See Resolution time 解析时间

system timing. See Timing analysis 系统时序，另见时序分析  
Timing analysis, 141–151: 时序分析  
 calculating cycle time. See Setup time constraint 计算周期时间，另见建立时间约束  
 hold time constraint. See Hold time constraint保持时间约束  
 max-delay constraint. See Setup time constraint最大延时约束，另见建立时间约束  
 min-delay constraint. See Hold time constraint最小延时约束，另见保持时间约束  
 multi-cycle processor, 407–408 多周期处理器  
 pipelined processor, 428流水线处理器  
 setup time constraint. See Setup time constraint建立时间约束  
 single-cycle processor, 388–389单周期处理器  
 with clock skew. See clock skew时钟偏移  
TLB. See Translation lookaside buffer：地址转换后备缓冲  
Trace cache, 463：跟踪缓存  
Transistors, 26–34：晶体管  
 bipolar, 26 双极  
 CMOS, 26–33  
 gates made from, 31–34 门  
 latches and flip-flops, 116–117 锁存器和触发器  
 MOSFETs, 26  
 nMOS, 28–34, 29–33  
 pMOS, 28–34, 29–33  
 pseudo-nMOS, 33–34伪nMOS  
 ROMs and PLAs, 279–280：ROM和PLA  
 transmission gate, 33  
Transistor-Transistor Logic (TTL), 25–26, 597–598: 晶体管－晶体管逻辑  
Translating and starting a program, 337–342, 338: 转换和开始执行程序  
Translation lookaside buffer (TLB), 502–503: 地址转换后备缓冲  
Transmission Control Protocol and: 传输控制协议  
Internet Protocol (TCP/IP), 561  
Transmission gates, 33: 传输门  
Transmission lines, 602–615：传输线  
 characteristic impedance (Z0), 612–613：特性阻抗(Z0)  
 derivation of, 612–613来源  
 matched termination, 604–606：匹配终端  
 mismatched termination, 607–610不匹配终端  
 open termination, 606–607开路终端  
 reflection coefficient (kr), 613–614反射系数(kr)  
 derivation of, 613–614来源  
 series and parallel terminations, 610–612 串联和并联终端  
 short termination, 607 短路终端  
 when to use, 610 何时使用  
Transparent latch. See D latch：透明锁存器，另见D锁存器  
Traps, 343：自陷  
Tristate buffer, 74–75, 187：三态缓冲器  
 HDL for, 186–187  
 multiplexer built using, 84–85, 91–93 用于构建多路选择器  
Truth tables, 20真值表  
 ALU decoder, 383, 384：ALU译码器  
 multiplexer, 83多路选择器  
 seven-segment display decoder, 79七段显示译码器  
 SR latch, 111, 112：SR锁存器  
 with don’t cares, 69, 81–83, 205带无关项  
 with undefined and floating inputs, 187–188带不确定和浮空输入  
TSOP. See Thin small outline package: 薄型小尺寸封装  
TTL. See Transistor-Transistor Logic: 晶体管-晶体管逻辑  
Two-bit dynamic branch predictor, 447: 双位动态分支预测  
Two-cycle latency of lw, 418：lw的两周期延时  
Two-level logic, 69: 双电平逻辑  
Two’s complement numbers, 16–18：2的补码  
typedef, 653–654

U  
UART. See Universal Asynchronous Receiver Transmitter: UART，另见通用异步收发器  
Unconditional branches, 315–316: 无条件分支  
Undefined instruction exception, 343–344, 440–443：未定义指令异常  
Unicode, 322   
Unit under test (UUT), 220: 被测单元(UUT)  
Unity gain points, 24单位增益点  
Universal Asynchronous Receiver Transmitter (UART), 521–527：通用异步收发器(UART),  
 hardware handshaking, 523 硬件握手  
 STA register, 524：STA寄存器  
Universal Serial Bus (USB), 270, 523, 559–560：通用串行总线(USB)  
 USB 1.0, 560  
 USB 2.0, 560  
 USB 3.0, 560  
Unsigned multiplier, 217：无符号乘法器  
Unsigned numbers, 18：无符号数  
USB. See Universal Serial Bus：USB，另见通用串行总线  
USB links, 563–564：USB链接  
 FTDI, 563  
 UM232H module, 564: UM232H模块  
Use bit (U), 490使用位(U)

V  
Valid bit (V), 484：有效位(V)  
Vanity Fair (Carroll), 76  
Variables in C, 629–633：C语言中的变量  
 global and local, 631–632全局和局部  
 initializing, 633初始化  
 primitive data types, 630–631基本数据类型  
Variable-shift instruction, 313 变量移位指令  
VCC , 23. See also Supply voltage, VDD：VCC，另见电源电压、VDD  
VDD, 22, 23. See also Supply voltage：VDD，另见电源电压  
Vector processor, 447：向量处理器  
Verilog. See SystemVerilog：Verilog，另见SystemVerilog  
Very High Speed Integrated Circuits (VHSIC), 175. See also VHDL：VHSIC ，另见VHDL  
VGA. See VGA monitor：VGA显示器  
VGA (Video Graphics Array) monitor, 541–547：VGA（视频图形阵列）显示器  
 connector pinout, 543接口引脚  
 driver for, 544–547 驱动程序  
VHDL. See VHSIC Hardware Description Language: VHDL，另见VHSIC硬件描述语言  
VHSIC. See Very High Speed Integrated Circuits: VHSIC  
VHSIC Hardware Description Language (VHDL), 173–175: VHSIC硬件描述语言(VHDL)  
 accessing parts of busses, 188, 192 访问总线部件  
 bad synchronizer with blocking assignments, 209 使用阻塞赋值的错误的同步器  
 bit swizzling, 188 位交叉混合  
 blocking and nonblocking assignment, 199–200, 205–208 阻塞和非阻塞赋值  
 case statements, 201–202, 205：case语句  
 combinational logic using, 177–193, 198–208, 217–220 组合逻辑  
 comments, 180 注释  
 conditional assignment, 181–182 条件语句  
 data types, 213–217 数据类型  
 decoders, 202–203, 219 译码器  
 delays (in simulation), 189 延时（在仿真中）  
 divide-by-3 FSM, 210–211 除以3 FSM  
 finite state machines (FSMs), 209–213 : 有限状态机  
 Mealy FSM, 213  
 Moore FSM, 210, 212  
 full adder, 184 全加器  
 using always/process, 200 使用always/process  
 using nonblocking assignments, 208 使用非阻塞赋值  
 history of, 175 历史  
 if statements, 202–205：if语句  
 internal signals, 182–184 内部信号  
 inverters, 178, 199 反相器  
 latches, 198 锁存器  
 logic gates, 177–179:逻辑门  
 multiplexers, 181–183, 190–193, 218–219: 多路选择器  
 multiplier, 217：乘法器  
 numbers, 185–186 数字  
 operators, 185 运算符  
 parameterized modules, 217–220：参数化模块  
 N:2N decoder, 219：N:2N 译码器  
 N-bit multiplexers, 218–219：N位多路选择器  
 N-input AND gate, 220：N输入与门  
 priority circuit, 204: 优先级电路  
 using don’t cares, 205 使用无关项  
 reduction operators, 180–181 缩减运算符  
 registers, 193–197 寄存器  
 enabled, 196 使能  
 resettable, 194–196 复位  
 sequential logic using, 193–198, 209–213 时序逻辑  
 seven-segment display decoder, 201七段显示译码器  
 simulation and synthesis, 175–177仿真和综合  
 structural models, 190–193 结构模型  
 synchronizer, 197 同步器  
 testbench, 220–224, 437–438 测试程序  
 self-checking, 222 自测试  
 simple, 221 简单  
 with test vector file, 223–224带测试向量  
 tristate buffer, 187 三态缓冲  
 truth tables with undefined and floating inputs, 187, 188 带不确定和浮空输入的真值表  
 z’s and x’s, 186–188, 205：z和x  
Video Graphics Array (VGA). See VGA monitor视频图形阵列(VGA)，另见VGA显示器  
Virtual address, 497虚拟地址  
 space, 503 :空间  
Virtual memory, 478, 496–506：虚拟内存  
 address translation, 497–500地址转换  
 cache terms comparison, 497缓存术语比较  
 memory protection, 503内存保护  
 multilevel page tables, 504–506多级页表  
 page fault, 497页面失效  
 page number, 498页码  
 page offset, 498页偏移  
 page table, 500–501页表  
 pages, 497页  
 replacement policies, 504替换策略  
 translation lookaside buffer (TLB), 502–503地址转换后备缓冲  
 write policy, 494–495写策略  
 x86, 567. See also x86  
Virtual page number (VPN), 499: 虚拟页码(VPN)  
Virtual pages, 497: 虚拟页  
VSS, 23

W  
Wafers, 28硅片  
Wait states, 564: 等待状态  
Wall, Larry, 20   
WAR. See Write after read：WAR，另见读取后写入  
WAW. See Write after write：WAW，另见写入后写入  
Weak pull-up, 33弱上拉  
Weird number, 18怪异数  
While loops, 318–319, 641：while循环  
White space, 180空格  
Whitmore, Georgiana, 7   
Wi-Fi, 561   
Wire, 67：导线  
Wireless communication, Bluetooth, 547–548无线通信，蓝牙  
Word-addressable memory, 301, 302：字可寻址存储器  
Wordline, 264字线  
Write after read (WAR) hazard, 451–453. See also Hazards读取后写入（WAR）冲突，另见冲突  
Write after write (WAW) hazard, 451写入后写入（WAW）冲突  
Write policy, 494–495写策略  
 write-back, 494–495写回  
 write-through, 494–495写直达

X  
X. See Contention, Don’t care：X，另见竞争、无关项  
x86  
 architecture, 347–355体系结构  
 branch conditions, 352分支条件  
 instruction encoding, 352–354,353指令编码  
 instructions, 350–352, 351指令  
 memory addressing modes, 349内存寻址模式  
 operands, 348–350操作数  
 registers, 348寄存器  
 status flags, 350状态标志  
 vs. MIPS, 348和MIPS比较  
 cache systems, 564–567缓存系统  
 memory system, evolution of, 565存储器系统，演化  
 microarchitecture, 458–465微结构  
 evolution of, 458–459演化  
 programmed I/O, 567–568可编程I/O  
 registers, 348寄存器  
 virtual memory, 567虚拟内存  
 protected mode, 567保护模式  
 real mode, 567实模式  
Xilinx FPGA, 274–276  
XNOR gate, 21–22: 同或门  
XOR gate, 21: 异或门  
xor, 311  
xori, 311–312

Z  
Z. See Floating：Z，另见浮空  
Zero extension, 250, 308, 311–312, 34零扩展